**Quote # QUO0000007626 (Rev 0)**

**ERP Number: 11629**

**Date: August 24th, 2023**

|  |  |
| --- | --- |
| Prepared For: | Presented By: |
| Bulldog Fire Apparatus | Bulldog Fire Apparatus |
| 17 Winter St | 17 Winter St. |
| Woodville, MA 01784 | Woodville, MA 01784 |
| Phone: (508) 435-4054 | Phone: (508) 435-4054 |
|  |  |

| **Option** | **QTY** | **Description** |
| --- | --- | --- |
| **BOILERPLATE** | | |
| PO00025823 | 1 | DESIGN CLAUSE |
| **GENERAL INFORMATION** | | |
| PO00011030 | 1 | PROPOSED BY BULLDOG FIRE APPARATUS |
| PO00011181 | 1 | COMPLETION INFORMATION |
| PO00011182 | 1 | FMVSS REQUIREMENT |
| PO00011183 | 1 | RECORDS |
| PO00011186 | 1 | GENERAL CONSTRUCTION |
| PO00011188 | 1 | PRODUCT LIABILITY |
| PO00011192 | 1 | PAINT CERTIFICATION |
| PO00011081 | 1 | PROPOSED SERVICE BY BULLDOG FIRE apparatus |
| PO00023879 | 1 | PRICES & PAYMENTS |
| PO00010973 | 1 | FAIR ETHICAL & LEGAL COMPETITION |
| PO00010976 | 1 | MATERIAL & WORKMANSHIP |
| PO00010978 | 1 | CONTRACT ADMINISTRATOR |
| PO00010979 | 1 | APPROVAL DRAWING |
| PO00010981 | 1 | DELIVERY |
| PO00025825 | 1 | INSTRUCTION MANUALS - usb |
| PO00011002 | 1 | PRODUCTION LEVEL ELECTRICAL DRAWINGS |
| PO00010982 | 1 | VEHICLE FLUID PLATE |
| PO00010983 | 1 | PRE-DELIVERY SERVICE |
| PO00010988 | 1 | EXACT BLUEPRINT WITH BID |
| PO00010990 | 1 | FAMA MEMBERSHIP |
| PO00010992 | 1 | MANUFACTURED IN UNITED STATES |
| PO00010997 | 1 | AMP DRAW REPORT |
| PO00010999 | 1 | SAFETY VIDEO |
| PO00011001 | 1 | COOPERATIVE PURCHASING |
| PO00027003 | 1 | VEHICLE TRANSPORTATION |

|  |  |  |
| --- | --- | --- |
| **DIMENSIONS** | | |
| PO00009792 | 1 | CRITICAL OVERALL HEIGHT REQUIREMENT – shall not exceed 12’ |
| PO00009794 | 1 | !!! CRITICAL OVERALL LENGTH REQUIREMENT – Shall not exceed 39’ |
| **NFPA REQUIREMENTS** | | |
| PO00011070 | 1 | NFPA 1901 GENERAL INFORMATION |
| PO00026614 | 1 | NFPA TREAD PLATE STEPPING/STANDING/WALKING SURFACE CERTIFICATION |
| PO00026616 | 1 | NON-EMBOSSED VERTICAL TREAD PLATE |
| PO00011005 | 1 | "AERIAL FIRE APPARATUS" NFPA 2016 CHAPTERS OF COMPLIANCE |
| PO00011169 | 1 | NFPA "CHAPTER 16" FIRE PUMP REQUIREMENTS |
| PO00011171 | 1 | NFPA "CHAPTER 18" {WATER TANKS} REQUIREMENTS |
| PO00011174 | 1 | NFPA "CHAPTER 22" {110 VOLT SYSTEM} REQUIREMENTS |
| **UL TESTING** | | |
| PO00025814 | 1 | THIRD PARTY TESTING |
| PO00024157 | 1 | 120 / 240 VOLT ELECTRICAL SYSTEM TESTING |
| PO00025850 | 1 | THIRD PARTY LINE VOLTAGE TESTING |
| **CAB MODEL AND DESIGN** | | |
| PO00025687 | 1 | SEVERE SERVICE CAB |
| PO00001589 | 1 | ALUMINUM CONSTRUCTION |
| PO00010253 | 1 | SEVERE SERVICE cab CRASH TESTING |
| **CAB LENGTH** | | |
| PO00008863 | 1 | SEVERE SERVICE CAB – 100” wide / xmfd (59-1/2”) |
| **CAB ROOF TYPE** | | |
| PO00012638 | 1 | 10" RAISED ROOF With 10" NOTCH OVER CREW area |
| PO00012643 | 1 | 52" WIDE NOTCH AERIAL RAISED ROOF |
| PO00009790 | 1 | TREAD PLATE OVERLAY ON CAB ROOF |
| PO00026121 | 1 | INTEGRAL CAB ROOF DRIP RAIL |
| **CAB STEPS** | | |
| PO00012134 | 1 | BATTERY ACCESS DOORS – each side REAR STEP WELLS |
| PO00010666 | 1 | CAST ANTI-SLIP ENTRY STEPS FOR FULL LENGTH DOORS |
| **CAB DOORS** | | |
| PO00001628 | 1 | FULL LENGTH CAB DOORS |
| PO00012478 | 1 | hd casted DOOR LATCHES |
| PO00012476 | 1 | KEY MODEL #751 |
| PO00001654 | 1 | ELECTRIC WINDOWs |
| PO00001659 | 1 | FULL HEIGHT INTERIOR DOOR PANELS - BRUSHed ALUMinum |
| PO00024908 | 1 | ORALITE CHEVRONS ON INTERIOR OF CAB DOOR PANELS |
| **CAB GLASS** | | |
| PO00010304 | 1 | WINDSHIELD |
| PO00025656 | 1 | WINDSHIELD WIPERS & WASHERS |
| PO00010308 | 1 | NON-SLIDING SIDE VIEWING WINDOWS |
| PO00001688 | 1 | DARK TINT WINDOWS, SIDE VIEWING, REAR DOORS |
| **CAB GRAB RAILS** | | |
| PO00001695 | 1 | HANSEN KNURLED ALUMINUM LIGHTED exterior GRAB RAILS |
| PO00001704 | 1 | WHEELABRATED INTERIOR GRAB HANDLES |
| PO00010627 | 1 | INTERIOR "A" & "C" POST GRAB HANDLES - BALL-BURNISHED |
| PO00010631 | 1 | INTERIOR GRAB RAILS - REAR CREW DOORS - BALL-BURNISHED |
| **CAB GRILLES AND OPTIONS** | | |
| PO00010617 | 1 | FRONT CAB GRILLE - SQUARE POLISHED STAINLESS STEEL |
| PO00025607 | 1 | SIDE CAB GRILLES - RECTANGLE STAINLESS STEEL |
| **CAB EXTERIOR** | | |
| PO00010591 | 1 | EXTERIOR REAR WALL TREAD PLATE OVERLAY |
| PO00001718 | 1 | aluminum CAB WHEEL WELL LINERS |
| PO00001720 | 1 | ALUMINUM CAB FENDERETTES |
| PO00010933 | 1 | FRONT MUD FLAPS |
| **MIRRORS** | | |
| PO00025657 | 1 | VELVAC MIRRORS " WEST COAST" HEATED / REMOTE with CONVEX SPOT |
| PO00025677 | 1 | MIRROR CONTROL |
| **CAB INTERIOR** | | |
| PO00011699 | 1 | cab DOOR WIDTH |
| PO00010643 | 1 | INTERIOR TRIM - GRAY DURAWEAR |
| PO00002964 | 1 | INTERIOR CAB WALL UPHOLSTERY – gray durawear |
| PO00010318 | 1 | BARYFOL FLOORING |
| PO00010317 | 1 | 1" ACOUSTICAL INSULATION |
| PO00011692 | 1 | ENGINE ENCLOSURE upholstery – gray durawear |
| PO00026126 | 1 | S2020 ENGINE ENCLOSURE ACCESS |
| PO00026118 | 1 | HD MILCUT SOUNDPROOFING / INSULATION PACKAGE UNDER ENGINE ENCLOSURE |
| PO00011646 | 1 | HD SOUNDPROOFING / INSULATION BETWEEN UPHOLSTERY & ENGINE ENCLOSURE |
| PO00011647 | 1 | ENGINE ENCLOSURE MOUNTING PANEL |
| PO00011657 | 1 | MOUNTING PLATE ON ENGINE ENCLOSURE FORWARD OF MAP BOX |
| PO00012475 | 1 | SUN VISORS - PADDED VINYL |
| PO00024654 | 1 | OVERHEAD FABRICATED CENTER THREE WING dash PANEL |
| **FRONT SEATING** | | |
| PO00012071 | 1 | SEAT AND SEAT BELT ANCHOR TESTING |
| PO00011311 | 1 | STORAGE COMPARTMENTS UNDER FRONT SEATS |
| PO00001779 | 1 | DRIVER SEAT - VALOR abts AIR SUSPENSION |
| PO00001841 | 1 | OFFICERS SEAT - VALOR abts FIXED BASE SCBA seat |
| PO00001847 | 1 | IMMI SMARTDOCK SCBA BRACKET – officer seat |
| PO00022634 | 1 | VALOR HORIZONTAL SLIDE ADJUSTMENT - OFFICER SEAT |
| **REAR FACING SEATS** | | |
| PO00001866 | 1 | driver side OUTBOARD REAR FACING crew SEAT - VALOR abts DYNAMIC CAVITY SCBA seat |
| PO00001871 | 1 | IMMI SMARTDOCK SCBA BRACKET – driver side OUTBOARD rear facing crew seat |
| PO00001890 | 1 | officer side outboard rear facing crew seat - valor abts dynamic cavity scba seat |
| PO00001895 | 1 | IMMI SMARTDOCK SCBA BRACKET – officer side OUTBOARD rear facing crew seat |
| **FORWARD FACING SEATS** | | |
| PO00023973 | 1 | two-(2) VALOR aBTS center FORWARD FACING scba seats |
| PO00022708 | 1 | center forward facing crew seats – FLIP-UP SEAT base |
| PO00022799 | 1 | IMMI SMARTDOCK SCBA BRACKET – two-(2) center forward facing crew seats |
| **SEATING OPTIONS** | | |
| PO00002002 | 1 | CENTER SEAT BASE WITH COMPARTMENTS - PAINTed DOORS |
| PO00024054 | 1 | SEAT ADJUSTMENT NOTICE |
| PO00008888 | 1 | VALOR SEATING MATERIAL - BLACK CORDURA |
| **VEHICLE SAFETY SYSTEM** | | |
| PO00025679 | 1 | CLASS ONE VEHICLE DATA RECORDER |
| PO00025680 | 1 | CLASS ONE SEAT BELT WARNING SYSTEM - UP TO 6 POSITIONS |
| PO00010780 | 1 | SIX (6) SEATING POSITIONS |
| **MISC INTERIOR CAB OPTIONS** | | |
| PO00010690 | 1 | COMPUTER TERMINAL IN FRONT OF OFFICER |
| **HVAC** | | |
| PO00025609 | 1 | HEATER / DEFROSTER & ACCESSORIES |
| PO00002176 | 1 | PAINT ROOF MOUNTED AIR CONDITIONER UNIT |
| PO00025689 | 1 | HVAC CONTROLS |
| PO00002179 | 1 | AUXiliary HEATERS UNDER REAR FACING seats |
| PO00026197 | 1 | ACTIVE AIR PURIFICATION SYSTEM |
| **CAB TILT SYSTEM** | | |
| PO00010681 | 1 | CAB TILT SYSTEM |
| PO00002182 | 1 | AUXILIARY MANUAL CAB LIFT BACKUP SYSTEM |
| PO00002186 | 1 | CAB TILT SECONDARY SAFETY LOCK |
| PO00002189 | 1 | PARKING BRAKE / CAB TILT INTERLOCK |
| **FRAME ASSEMBLY** | | |
| PO00024080 | 1 | 110,000 PSI FRAME TRIPLE FRAME RAIL |
| PO00023914 | 1 | AERIAL TRAVEL SUPPORT |
| PO00024146 | 1 | GALVANIZED TRIPLE FRAME RAILS |
| **FRONT BUMPER** | | |
| PO00002195 | 1 | 12" PAINTED 3/8" STEEL fornt BUMPER |
| PO00002200 | 1 | 10" FRONT BUMPER EXTENSION WITH TREAD PLATE GRAVEL SHIELD |
| **FRONT BUMPER ACCESSORIES** | | |
| PO00002309 | 1 | TWO (2) PAINTED TOW EYES BELOW FRONT BUMPER |
| **FRONT AXLE** | | |
| PO00024470 | 1 | 24,000# FRONT AXLE STEERTEK with DISC BRAKES |
| **STEERING SYSTEM** | | |
| PO00010598 | 1 | DUAL SHEPPARD POWER STEERING GEARS |
| PO00010603 | 1 | STEERING COLUMN - CLOCK SPRING "NARROW" |
| PO00010604 | 1 | 18" 4-spoke STEERING WHEEL |
| **REAR AXLE** | | |
| PO00010594 | 1 | DRIVER CONTROLLED DIFFERENTIAL LOCK |
| PO00002385 | 1 | 58,000# TANDEM REAR AXLE MERITOR RT-58-185 |
| PO00002390 | 1 | 16.5" X 8.6" S-CAM BRAKES - MERITOR REAR TANDEM With AUTO SLACK ADJUSTERS |
| PO00023915 | 1 | VEHICLE TOP SPEED - NFPA STATEMENT |
| PO00002425 | 1 | HENDRICKSON HN FR-582 RUBBER BLOCK SUSPENSION |
| **FRONT WHEELS AND TIRE** | | |
| PO00002489 | 1 | FRONT WHEELS - DURABRIGHT ALUMINUM, 22.5 X 12.25 |
| PO00002491 | 1 | FRONT WHEELS LUG AND HUB TRIM |
| PO00002510 | 1 | FRONT tires - MICHELIN 425/65R22.5 L 24,396# XZY3 WB MIXED tread pattern |
| **REAR TIRES AND WHEELS** | | |
| PO00002550 | 1 | REAR WHEELS - DURABRIGHT ALUMINUM, 22.5 X 9 |
| PO00002554 | 1 | REAR WHEELS LUG AND HUB TRIM |
| PO00002605 | 1 | REAR tires - MICHelin 315/80R22.5 L 70,792# XDN2 GRIP TRACtion tread - 75MPH |
| PO00002626 | 1 | TIRE PRESSURE MONITORING - LED VALVE STEM CAPS |
| **BRAKE AND AIR SYSTEM** | | |
| PO00010545 | 1 | BRAKE SYSTEM - TANDEM AXLE CHASSIS |
| PO00010547 | 1 | ABS BRAKING FOR TANDEM REAR AXLE CHASSIS |
| PO00002442 | 1 | ELECTRONIC STABILITY CONTROL (ESC) WITH auto traction control (ATC) |
| PO00002454 | 1 | AIR RESERVOIRS 7100 CUBIC INCH TANDEM AXLE With 1127 CUBIC INCH ADDITIONAL TANK - COLOR CODED |
| PO00002457 | 1 | STAINLESS STEEL AIR TANK BRACKETS - (5 TANKS) |
| PO00010713 | 1 | HEATED AUTOMATIC MOISTURE ejectors |
| PO00002458 | 1 | 1/4 TURN DRAIN VALVES ON ALL AIR TANKS - SIDE OF VEHICLE |
| PO00002463 | 1 | MERITOR / WABCO SYSTEM SAVER #1200 heated AIR DRYER |
| PO00010321 | 1 | COLOR CODED SYNFLEX BRAKE LINES With QUICK RELEASE FITTINGS |
| PO00011823 | 1 | AIR COMPRESSOR -WABCO - ALL CUMMINS ENGINES |
| PO00011824 | 1 | BRAKE TREADLE VALVE |
| PO00002466 | 1 | PARKING BRAKE CONTROL with all wheel lock-up - NEAR DRIVER |
| PO00025507 | 1 | BLUE SEA 12-Volt / 125PSI AIR COMPRESSOR |
| PO00026194 | 1 | 12-VOLT AIR COMPRESSOR SHORELINE RELAY |
| **ENGINE** | | |
| PO00026114 | 1 | CUMMINS X15 605 HP AT 1600 RPM, 1850 FT. LBS. TORQUE AT 1150 RPM |
| PO00010717 | 1 | ENGINE IQA CERTIFICATION - X15 |
| PO00002712 | 1 | SECONDARY BRAKING - ENGINE COMPRESSION BRAKE |
| PO00010493 | 1 | ENGINE AIR CLEANER |
| PO00010494 | 1 | EMBER SEPARATOR |
| PO00010495 | 1 | ACCELERATOR PEDAL |
| PO00010496 | 1 | REMOTE THROTTLE & INTERLOCK HARNESS |
| **COOLING SYSTEM** | | |
| PO00011703 | 1 | COOLING / RADIATOR system |
| PO00010649 | 1 | COOLING SYSTEM CRITERIA |
| PO00010650 | 1 | TRANSMISSION COOLER |
| PO00010651 | 1 | RADIATOR CROSS MEMBER |
| PO00011685 | 1 | CHARGED AIR COOLER |
| PO00011686 | 1 | COOLANT FAN With CLUTCH |
| PO00002710 | 1 | HEATER AND COOLANT HOSES / PIPING |
| PO00023874 | 1 | LOW COOLANT INDICATOR |

|  |  |  |
| --- | --- | --- |
| **TRANSMISSION** | | |
| PO00002720 | 1 | ALLISON 4000EVS TRANSMISSION with COMPRESSION BRAKE |
| PO00002732 | 1 | SIX (6) SPEED AUTOMATIC TRANSMISSION |
| PO00002736 | 1 | ALLISON TRANSMISSION ELECTRONIC TOUCH PAD SHIFTER IN CAB |
| PO00010553 | 1 | TRANSMISSION OIL LEVEL SENSOR |
| PO00010554 | 1 | ALLISON PARK TO NEUTRAL |
| PO00010555 | 1 | ALLISON PRESELECT PROGRAMMING |
| PO00002741 | 1 | PRESELECT PROGRAMMED FOR 3RD GEAR |
| PO00023876 | 1 | TES 295 SYNTHETIC TRANSmission FLUID |
| PO00010794 | 1 | TRANSMISSION LOCK-UP |
| **DRIVELINES AND OPTIONS** | | |
| PO00010565 | 1 | DRIVE LINES DANA-SPICER #1810 SERIES |
| **EXHAUST SYSTEM** | | |
| PO00002748 | 1 | 5 GALLON DEF TANK |
| PO00012469 | 1 | DIESEL EXHAUST FLUID LEVEL GAUGE |
| PO00010556 | 1 | EXHAUST SYSTEM - DPF & SCR inline SYSTEM |
| PO00010558 | 1 | STAINLESS STEEL EXHAUST TAILPIPE / OUTLET – officer side termination |
| **FUEL SYSTEM** | | |
| PO00002770 | 1 | STAINLESS STEEL FUEL TANK - 65 GALLON |
| PO00010567 | 1 | STAINLESS STEEL FUEL TANK STRAPS |
| PO00010568 | 1 | FUEL TANK MOUNTING STRAP ISOLATION MATERIAL |
| PO00010569 | 1 | FUEL LINES - FIBER REINFORCED HOSE |
| PO00010570 | 1 | CUMMINS FUEL-WATER SEPARATOR |
| PO00010572 | 1 | FUEL PUMP ELECTRIC re-primer |
| PO00026203 | 1 | FUEL POCKET - DRIVER SIDE REAR WHEEL WELL PANEL |
| **CHASSIS ELECTRICAL HARNESSES AND TESTING** | | |
| PO00010721 | 1 | PUMPER BODY ELECTRICAL |
| PO00011797 | 1 | CUSTOM CHASSIS ELECTRICAL SYSTEM |
| PO00022590 | 1 | 12-VOLT ELECTRICAL SYSTEM TESTING |
| PO00011798 | 1 | CUSTOM CHASSIS WIRING INSTALLATION |
| PO00011799 | 1 | DIRECT BATTERY GROUNDING STRAP |
| PO00011800 | 1 | EMI / RFI PROTECTION |
| PO00011805 | 1 | SEQUENCER |
| **ELECTRICAL SYSTEM CONTROL TYPE** | | |
| PO00010662 | 1 | MULTIPLEX CONTROL PUMP SHIFT SWITCH |
| PO00010255 | 1 | MULTIPLEX ELECTRICAL SYSTEM |
| PO00011807 | 1 | INTER-LOCK MODULE FOR MULTIPLEX SYSTEM |
| **ALTERNATOR** | | |
| PO00002801 | 1 | DELCO REMY 55SI 430 AMP BRUSHLESS ALTERNATOR |
| **BATTERIES** | | |
| PO00026645 | 1 | SIX-(6) EXIDE GROUP 31 950 CCA batteries - SX31XHD |
| PO00012455 | 1 | steeel BATTERY STORAGE |
| PO00012459 | 1 | BATTERY BOX COVERs |
| PO00012452 | 1 | COLE HERSEE BATTERY JUMPER STUDS – Driver SIDE CAB STEP well |
| PO00012461 | 1 | BATTERY DISCONNECT SWITCH |
| **SHORELINE AND CHARGER SYSTEM** | | |
| PO00025504 | 1 | BLUE SEA 120 VOLT 20 AMP SURE EJECT FOR BATTERY CHARGER |
| PO00025508 | 1 | RED COVER FOR BLUE SEA SURE EJECT RECEPTACLE |
| PO00002839 | 1 | SHORELINE LOCATION - ADJACENT TO DRIVER'S DOOR |
| PO00022630 | 1 | SHORELINE RECEPTACLE LABEL |
| PO00025505 | 1 | BLUE SEA #7532 40 AMP P12 BATTERY CHARGER |
| PO00025634 | 1 | BLUE SEA EV BATTERY CHARGER DISPLAY |
| PO00012313 | 1 | 120-volt AUTOMATIC TRANSFER SWITCH |
| **CAB INTERIOR 12-VOLT POWER ACCESSORIES** | | |
| PO00025600 | 1 | BLUE SEA #4365 ACCESSORY PANEL |
| PO00022420 | 1 | 120-VOLT POWER STRIP REAR CREW AREA WIRED TO SHORELINE |
| PO00010730 | 1 | POWER AND GROUND STUD FOR ACCESSORIES IN DASH |
| PO00012536 | 1 | BLUE SEA FUSE BLOCK - 12 CIRCUIT IN REAR CREW AREA |
| PO00012534 | 1 | BLUE SEA FUSE BLOCK - 12 CIRCUIT BEHIND OFFICER SEAT |
| PO00026778 | 1 | USB POWER POINT - REAR FACING SEATING AREA |
| PO00010732 | 1 | IGNITION STUD - REAR CREW AREA |
| **CAB INTERIOR LIGHTING** | | |
| PO00002894 | 1 | WHELEN 6" ROUND WHITE / RED LED INTERIOR LIGHTS |
| PO00024655 | 1 | led INNER CAB DOOR FLASHERS - WHELEN DOOR STRIP LIGHTs |
| PO00011819 | 1 | ENGINE COMPARTMENT WORK LIGHTS - TECNIQ LED |
| **CAB INSTRUMENT PANEL AND CONTROLS** | | |
| PO00011695 | 1 | DASH & CENTER CONSOLE |
| PO00024139 | 1 | CAB DASH PANELS |
| **CONTROLS SWITCHING** | | |
| PO00010634 | 1 | STANDARD #MATM RADIO ANTENNA |
| PO00012297 | 1 | CONTROL SWITCHING THROUGH MULTIPLEX screen |
| PO00010735 | 1 | HOSE BED WORK LIGHT SWITCH |
| PO00003391 | 1 | CONTROL SWITCHES IN CAB FOR LIGHT ABOVE WINDSHIELD |
| PO00003232 | 1 | CONTROL SWITCHES IN CAB FOR BEHIND FRONT CAB DOOR LIGHTS |
| PO00003234 | 1 | CONTROL SWITCH IN CAB FOR 12-Volt REAR OF BODY SCENE LIGHTS |
| **DRIVER OVERHEAD** | | |
| PO00025616 | 1 | TWELVE-(12) ADDITIONAL SWITCHES - DRIVER OVERHEAD ZONE |
| **GAUGE PANEL** | | |
| PO00011697 | 1 | DRIVER'S DASHBOARD PANEL |
| PO00022740 | 1 | DRIVER DASH - LCD VIRTUAL DISPLAY |
| **DRIVER LOWER WING** | | |
| PO00010551 | 1 | FAST IDLE ON DASH FOR ALL ELECTRONIC ENGINES |
| PO00025626 | 1 | SIX (6) ADDITIONAL SWITCHES - DRIVER LOWER WING ZONE |
| PO00010697 | 1 | ENGINE COMPRESSION BRAKE CONTROLS |
| PO00002774 | 1 | CLASS-1 ES-KEY ULTRAVIEW 780 DISPLAY |
| **OFFICER LOWER WING** | | |
| PO00025622 | 1 | SIX (6) ADDITIONAL SWITCHES - OFFICER LOWER WING ZONE |

|  |  |  |
| --- | --- | --- |
| **DRIVER LEFT KNEE** | | |
| PO00025678 | 1 | PUMP SHIFT CONTROL ON DRIVER LOWER LEFT KNEE PANEL |
| **CAMERAS SYSTEM** | | |
| PO00026078 | 1 | INVIEW 360™ HD VIDEO SYSTEM |
| **CAB DOT MARKER AND STEP LIGHTING** | | |
| PO00010733 | 1 | CUSTom CHASSIS LED MARKER LIGHTS |
| PO00003068 | 4 | CAB STEP LIGHTS - TECNIQ EON 3 LED |
| **HEADLIGHT AND FRONT DIRECTIONAL LIGHTING** | | |
| PO00002986 | 1 | DUAL MODULE With FEDERAL QL64Z-ARROW LED TURN SIGNAL & REQuired WARNing LIGHTs |
| PO00004075 | 1 | ALTERNATE FLASHING HEADLIGHT SYSTEM - WIG-WAGS |
| PO00024477 | 1 | DUAL HEADLIGHTS LED FIRETECH HIVIZ |
| PO00010729 | 1 | DAYTIME RUNNING LIGHTS |
| **CAB EXTERIOR 12-VOLT LIGHTING** | | |
| PO00003396 | 1 | WIRE UPGRADE FOR 12-Volt HIGH AMP LIGHT BROW LIGHT |
| PO00024441 | 1 | HIVIZ FIRETECH 80" BROW LIGHT With IML – 305 Watt 12-Volt, ABOVE WINDSHIELD |
| **WARNING LIGHT SYSTEMS** | | |
| PO00010755 | 1 | NFPA COMPLIANT WARNING LIGHT PACKAGE |
| PO00010757 | 1 | WARNING LIGHT FLASH PATTERN - NFPA FLASH PATTERN |
| PO00010756 | 1 | LIGHT PACKAGE ACTUATION / CONTROLS |
| PO00010759 | 1 | LIGHT PACKAGE NFPA CERTIFICATION |
| **UPPER WARNING LIGHT PACKAGE** | | |
| PO00003760 | 1 | upper zone A led warning lights - feDERAL LED 25” MINI NAVIGATOR light bars |
| PO00003803 | 1 | upper zone C led warning lights - FEDERAL QUADRAFLARE, 7X9 LED LIGHTS |
| PO00024573 | 1 | UPPER ZONE C WARNING LIGHT LENS - RED |
| PO00024593 | 1 | UPPER ZONE C WARNING LIGHT BEZEL - CHROME |
| PO00003813 | 1 | upper zone B/D FRONT led warning lights - FEDERAL QUADRAFLARE, 4X6 LED LIGHTS |
| PO00024575 | 1 | UPPER ZONE B/D FRONT WARNING LIGHT LENS - RED |
| PO00024595 | 1 | UPPER ZONE B/D FRT WARNING LIGHT BEZEL - CHROME |
| PO00003809 | 1 | upper zone B/D REAR led warning lights - FEDERAL QUADRAFLARE, 4X6 LED LIGHTS |
| PO00024577 | 1 | UPPER ZONE B/D REAR WARNING LIGHT LENS - RED |
| PO00024597 | 1 | UPPER ZONE B/D REAR WARNING LIGHT BEZEL - CHROME |
| **LOWER WARNING LIGHT PACKAGE** | | |
| PO00012072 | 1 | lower zone A FRONT led warning lights MOUNTING |
| PO00003982 | 1 | lower zone a FRONT led warning lights - FEDERAL QUADRAFLARE LED, 4X6 LED LIGHTS |
| PO00024579 | 1 | LOWER ZONE A WARNING LIGHT LENS - RED |
| PO00024599 | 1 | LOWER ZONE A WARNING LIGHT BEZEL - CHROME |
| PO00009828 | 1 | lower zone C REAR led warning lights - FEDERAL QUADRAFLARE LED, 4X6 LED LIGHTS |
| PO00024581 | 1 | LOWER ZONE C WARNING LIGHT LENS - RED |
| PO00012074 | 1 | lower zone B/D FRONT led warning lights MOUNTING |
| PO00003992 | 1 | lower zone B/D fRONT led warning lights - FEDERAL QUADRAFLARE LED, 4X6 LED LIGHTS |
| PO00024583 | 1 | LOWER ZONE B/D FRONT WARNING LIGHT LENS - RED |
| PO00024603 | 1 | LOWER ZONE B/D FRONT WARNING LIGHT BEZEL - CHROME |
| PO00003996 | 1 | lower zone b/D-LOWER MID led warning lights - FEDERAL QUADRAFLARE LED, 4X6 LED LIGHTS |
| PO00024585 | 1 | LOWER ZONE B/D MID WARNING LIGHT LENS - RED |
| PO00024605 | 1 | LOWER ZONE B/D MID WARNING LIGHT BEZEL - CHROME |
| PO00004000 | 1 | lower zone B/D SECONDARY MID led warning lights - FEDERAL QUADRAFLARE, 4X6 LED LIGHTS |
| PO00024589 | 1 | LOWER ZONE B/D MID SECONDARY WARNING LIGHT LENS - RED |
| PO00024609 | 1 | LOWER ZONE B/D MID SEC WARNING LIGHT BEZEL - CHROME |
| PO00004004 | 1 | lower zone B/D REAR led warning lights - FEDERAL QUADRAFLARE, 4X6 LED LIGHTS |
| PO00024587 | 1 | LOWER ZONE B/D REAR WARNING LIGHT LENS - RED |
| PO00024607 | 1 | LOWER ZONE B/D REAR WARNING LIGHT BEZEL - CHROME |
| **OUTRIGGER WARNING LIGHTS** | | |
| PO00013266 | 1 | FEDERAL 4X6, QUADRAFLARE LED LIGHTs ON (4) OUTRIGGER PANELS |
| PO00013270 | 1 | OUTRIGGER WARNING LIGHT ACTIVATION with PRIMARY WARNING lights |
| **VEHICLE GROUND LIGHTING** | | |
| PO00003295 | 1 | NFPA (4) TECNIQ #E10 LED GROUND LIGHTS BELOW CAB DOORS |
| PO00003296 | 1 | GROUND LIGHTS, 2 LED UNDER FRONT BUMPER FACING FORWARD - TECNIQ E10 |
| PO00003298 | 1 | GROUND LIGHTS, 2 LED BELOW PUMP PANEL RUNNING BOARD - TECNIQ E10 |
| PO00003300 | 1 | GROUND LIGHTS, 2 LED BELOW FRONT BODY CORNERS - TECNIQ E10 |
| PO00003301 | 1 | GROUND LIGHTS, 2 LED AT REAR BODY CORNERS - TECNIQ E10 |
| PO00009695 | 1 | CAB AND BODY GROUND LIGHTS ACTIVATE WITH PARKING BRAKE |
| PO00026831 | 1 | CAB AND BODY GROUND LIGHTS ACTIVATE WITH MASTER SWITCH IN CAB |
| **BODY ELECTRICAL HARNESS AND TESTING** | | |
| PO00022750 | 1 | AERIAL LADDER POWER SWITCH IN CAB |
| PO00011802 | 1 | CHASSIS DIAGNOSTICS SYSTEM |
| PO00011803 | 1 | VOLTAGE MONITORING SYSTEM - 12 VOLT |
| PO00011804 | 1 | INDICATOR LIGHT AND ALARM PROVE-OUT SYSTEM |
| PO00011806 | 1 | ELECTRICAL HARNESS INSTALLATION - 12 VOLT |
| PO00012671 | 1 | AERIAL BODY ELECTRICAL SYSTEM |
| PO00010753 | 1 | BODY ELECTRICAL HARNESS - ES-KEY |
| PO00010754 | 1 | POWER DISTRIBUTION MODULES FOR CLASS ONE ES-KEY SYSTEM |
| **COMPARTMENT LIGHTS** | | |
| PO00012441 | 1 | DOOR OPEN INDICATOR With INTEGRAL AUDIBLE ALARM |
| PO00009693 | 1 | DUNNAGE AREA LIGHTING - TECNIQ EON 3 |
| PO00011816 | 1 | COMPARTMENT LIGHT ACTIVATION |
| PO00003422 | 10 | COMPARTMENT LIGHTing – dual AMDOR LUMA BAR LED LIGHTING |
| **BODY DOT MARKER AND STEP LIGHTING** | | |
| PO00010734 | 1 | CUSTom BODY LED MARKER LIGHTS |
| PO00002998 | 1 | DOT MARKER LIGHTS FORWARD OF FRONT CAB DOOR |
| PO00002999 | 1 | MARKER / TURN LIGHTS - EAch SIDE OF BODY |
| PO00003003 | 1 | DOT MARKER LIGHTS - REAR OF BODY |
| PO00003007 | 1 | DOT AMBER REFLECTORS - SIDE OF BODY |
| PO00003008 | 1 | DOT RED REFLECTORS - REAR OF BODY |
| PO00026701 | 1 | TECNIQ #L10 LED LICENSE PLATE LIGHT |
| PO00012422 | 1 | BRITAX 6" ANGLED RUBBER LED LIGHT - REAR BODY CORNERS |
| PO00009410 | 1 | FEDERAL QUADRAFLARE LED BRAKE, REVERSE, & TURN With QUAD HOUSIng |
| PO00003075 | 2 | led BODY STEP LIGHTS - TECNIQ EON 3 |
| PO00003402 | 1 | PUMP ENCLOSURE WORK LIGHTS - TECNIQ LED |
| **BODY SCENE LIGHTING 12-VOLT** | | |
| PO00003106 | 1 | AMDOR LED STRIP HOSE BED LIGHT - FRONT HOSE BED WALL |
| PO00015934 | 1 | AERIAL ACCESS LADDER ILLUMINATION |
| PO00024726 | 1 | FIRETECH HIVIZ GUARDIAN LED SCENE LIGHTS BEHIND FRONT CAB DOORS |
| \*\*\*SPECIAL: SP00039366 | 1 | HIVIZ FT-B-27-ML3R-W MOUNTED AT REAR OF AERIAL BODY |
| PO00003244 | 1 | CAB SCENE LIGHTS TO BE ACTIVATED BY CAB DOORS |
| PO00003245 | 1 | REAR SCENE LIGHTS TO BE ACTIVATED BY REVERSE LIGHTS |
| **TRAFFIC ADVISOR** | | |
| PO00004174 | 1 | FEDERAL 31" LED "LATITUDE SIGNAL MASTER" LIGHT AT REAR OF BODY |
| PO00004193 | 1 | TRAFFIC ADVISOR MOUNTING ON REAR body SHEET |
| **GENERATOR** | | |
| PO00004288 | 1 | HARRISON PTO / HYDraulic GENerator - 10.0-MCR STEALTH SERIES, 10,000 WATT |
| PO00024160 | 1 | 120 & 240 VOLT WIRING METHODS |
| PO00004497 | 1 | GENerator LOCATION - TOP OF BODY |
| PO00004319 | 1 | GENERATOR RUNNING LIGHT (120 VOLT) ON CAB DASH |
| PO00012325 | 1 | HARRISON HOT SHIFT PTO |
| PO00012327 | 1 | DIGITAL QUAD METER FOR HARRISON GENERATOR |
| **CIRCUIT BREAKER PANEL** | | |
| PO00004323 | 1 | EIGHT (8) SPACE 100 AMP MAIN LUG LOAD CENTER |
| PO00004405 | 1 | LOCATE BREAKER PANEL DRIVER SIDE FRONT COMPARTMENT |
| PO00026694 | 1 | LINE VOLTAGE BREAKER TYPE - NON-GFCI/AFCI |
| **CORD REEL #1** | | |
| PO00008828 | 1 | HANNAY ECR-1616-17-18, 120 VOLT ELECTRIC CORD REEL |
| PO00021051 | 1 | CORD REEL LOCATION CEILING MOUNT OFFICER FRONT COMPARTMENT |
| PO00021071 | 1 | NO GUIDE ROLLER TO BE PROVIDED |
| PO00021067 | 1 | REWIND SWITCH - ADJACENT TO CORD REEL #1 |
| PO00009422 | 1 | 150 FEET OF 12/3 YELLOW CABLE FOR 120 VOLT REEL |
| PO00021153 | 1 | CIRCLE-D (20 TWIST) PF51GFCI-5 J-BOX ON END OF CABLE |
| PO00021154 | 1 | CIRCLE-D (20 TWIST) PF51GFCI-5P J-BOX WITH PIGTAIL |
| PO00021197 | 1 | TREAD PLATE JUNCTION BOX HOLDER |
| PO00021066 | 1 | CORD REEL CIRCUIT BREAKER REQUIREMENTS |
| PO00021074 | 1 | BALL STOP ON END OF CABLE |
| **AUDIBLE DOT** | | |
| PO00011814 | 1 | CHASSIS DOT HORN |
| PO00004204 | 1 | CODE 3 #CA360C BACK-UP ALARM - 107 DBA |
| **AIR HORN SYSTEM** | | |
| PO00024127 | 1 | DUAL CHROME AIR HORNS |
| PO00002946 | 1 | DUAL AIR HORNS RECESSED IN FRONT BUMPER |
| PO00026745 | 1 | AIR HORN CONTROL - CEILING MOUNTED LANYARD / STEERING WHEEL HORN BUTTON FOR DRIVER |
| PO00026731 | 1 | additional AIR HORN CONTROL - CEILING MOUNTED LANYARD FOR OFFICER |
| **ELECTRONIC SIREN AND SPEAKER** | | |
| PO00004208 | 1 | WHELEN #295SLSA1, 100-watt electronic siren |
| PO00004239 | 1 | ONE (1) WHELEN SA315P siren SPEAKER |
| PO00024983 | 1 | POLISHED STEEL ELECTRONIC SIREN SPEAKER GRILL |
| **MECHANICAL SIREN** | | |
| PO00012247 | 1 | FEDERAL Q2B SIREN - CAB FRONT |
| PO00012256 | 1 | Q2B MOUNT FULLY RECESSED INTO DRIVER SIDE OF BUMPER |
| PO00026752 | 1 | q2b SIREN BRAKE CONTROL for officer - DASH SWITCH |
| PO00026753 | 1 | q2b SIREN BRAKE CONTROL for driver - DASH SWITCH |
| PO00026761 | 1 | q2b SIREN CONTROL for driver - FLOOR SWITCH |
| PO00026763 | 1 | q2b SIREN CONTROL for officer - DASH SWITCH |
| **PUMP** | | |
| PO00004701 | 1 | HALE QMAX-XS 150 1500 GPM SINGLE STAGE PUMP |
| PO00010792 | 1 | PUMP RATIO |
| PO00009802 | 1 | PUMP MOUNTS - MID-SHIP PUMPS |
| **PUMP OPTIONS** | | |
| PO00009138 | 1 | HALE MECHANICAL PUMP SEAL |
| PO00009103 | 1 | HALE PUMP DRIVE UNIT - K GEARBOX |
| PO00010793 | 1 | PUMP SHIFT MANUAL OVERRIDE |
| PO00012078 | 1 | HALE PUMP SHIFT INDICATOR LIGHTS |
| PO00011537 | 1 | HALE alloy ANODE BLOCKS |
| PO00010750 | 1 | AUXILIARY ENGINE COOLER |
| **PRESSURE CONTROL** | | |
| PO00004810 | 1 | FIRE RESEARCH "PUMP BOSS" PBA400 PRESSURE GOVERNOR |
| PO00011415 | 1 | TASK FORCE TIPS #A18 SERIES INTAKE RELIEF VALVE |
| **PRIMER SYSTEM AND OPTIONS** | | |
| PO00009890 | 1 | TRIDENT "MANUAL" AIR PRIMING SYSTEM |
| **DRAINS AND OPTIONS** | | |
| PO00004825 | 1 | ROTARY MASTER DRAIN VALVE |
| PO00004830 | 1 | DRAINS/BLEEDER "INNOVATIVE CONTROLS" LIFT UP style |
| PO00004840 | 1 | SYNFLEX SUCTION, DISCHARGE, PRESSURE AND CONTROL LINES |
| **INTAKES** | | |
| PO00010965 | 1 | 6” SUCTION INLETS |
| PO00024018 | 1 | SHORT NECK MAIN PUMP SUCTION INLETS |
| PO00012076 | 1 | BEHIND PANEL MOUNT |
| PO00023976 | 1 | 6" NST INTAKE CAP - DRIVER SIDE |
| PO00023980 | 1 | 6" NST INTAKE CAP - OFFICER SIDE |
| **DRIVER SIDE AUXILIARY INTAKE** | | |
| PO00011333 | 1 | 2-1/2" DRIVER SIDE AUXiliary SUCTION INLET |
| PO00004970 | 1 | 2-1/2" ELKHART VALVE |
| PO00004984 | 1 | SWING CONTROL VALVE |
| **OFFICER SIDE AUXILIARY INTAKE** | | |
| PO00011335 | 1 | 2-1/2" OFFICER SIDE AUXiliary SUCTION INLET |
| PO00023916 | 1 | 2-1/2" ELKHART VALVE |
| PO00009373 | 1 | SWING CONTROL VALVe |
| **TANK TO PUMP** | | |
| PO00023881 | 1 | TANK TO PUMP 3” VALVE |
| PO00004999 | 1 | 3" AKRON #8800 stainless steel ball valve |
| PO00010956 | 1 | PUSH/PULL CONTROL |
| **TANK FILL** | | |
| PO00010962 | 1 | TANK FILL LINE 2" FROM PUMP |
| PO00005031 | 1 | 2" AKRON #8800 STAINLESS STEEL BALL VALVE |
| PO00009815 | 1 | PUSH/PULL CONTROL |
| **DRIVER SIDE DISCHARGE #1** | | |
| PO00012083 | 1 | DRIVER SIDE DISCHARGE #1 |
| PO00009226 | 1 | 2-1/2" AKRON #8800 STAINLESS STEEL BALL VALVE |
| PO00005039 | 1 | 2-1/2" STRAIGHT NST & 30-DEGREE NST ELBOW ADAPTER |
| PO00005050 | 1 | 2-1/2" NST PRESSURE VENTED CAP |
| PO00005084 | 1 | PUSH/PULL CONTROL |
| PO00005121 | 1 | INNOVATIVE CONTROLS LIQUID FILLED 2-1/2" PRESSURE GAUGE |
| **DRIVER SIDE DISCHARGE #2** | | |
| PO00012084 | 1 | DRIVER SIDE MAIN DISCHARGE #2 |
| PO00009304 | 1 | 2-1/2" AKRON #8800 STAINLESS STEEL BALL VALVE |
| PO00005145 | 1 | 2-1/2" STRAIGHT NST & 30-DEGREE NST ELBOW ADAPTER |
| PO00005156 | 1 | 2-1/2" NST PRESSURE VENTED CAP |
| PO00009303 | 1 | PUSH/PULL CONTROL |
| PO00005223 | 1 | INNOVATIVE CONTROLS LIQUID FILLED 2-1/2" PRESSURE GAUGE |
| **OFFICER SIDE DISCHARGE #1** | | |
| PO00012086 | 1 | OFFICER SIDE MAIN DISCHARGE #1 |
| PO00005281 | 1 | 4" AKRON #8840 VALVE |
| PO00005299 | 1 | 4" STRAIGHT NST ADAPTER |
| PO00005303 | 1 | 4" NST PRESSURE VENTED CAP |
| PO00005347 | 1 | 4" AKRON #9335 ELECTRIC VALVE CONTROL |
| PO00005370 | 1 | INNOVATIVE CONTROLS LIQUID FILLED 2-1/2" PRESSURE GAUGE |
| **OFFICER SIDE DISCHARGE #2** | | |
| PO00012087 | 1 | OFFICER SIDE DISCHARGE #2 |
| PO00005393 | 1 | 2-1/2" AKRON #8800 STAINLESS STEEL BALL VALVE |
| PO00005403 | 1 | 2-1/2" STRAIGHT NST & 30-DEGREE NST ELBOW ADAPTER |
| PO00005414 | 1 | 2-1/2" NST PRESSURE VENTED CAP |
| PO00005446 | 1 | PUSH/PULL CONTROL |
| PO00005482 | 1 | INNOVATIVE CONTROLS LIQUID FILLED 2-1/2" PRESSURE GAUGE |
| **CROSSLAY #1** | | |
| PO00000011 | 1 | CROSSLAY #1 - 1-1/2" |
| PO00000014 | 1 | CROSSLAY #1 CAPACITY - 200 FEET OF 1-3/4" HOSE |
| PO00000022 | 1 | CROSSLAY #1 - DOUBLE STACK HOSE DESIGN |
| PO00006565 | 1 | 1-1/2" NST CHICKSAN SWIVEL |
| PO00006572 | 1 | CROSSLAY #1 PLUMBING - 2" STAINLESS STEEL PIPING |
| PO00006578 | 1 | 2" AKRON #8800 STAINLESS STEEL BALL VALVE |
| PO00006592 | 1 | PUSH/PULL CONTROL |
| PO00006625 | 1 | INNOVATIVE CONTROLS LIQUID FILLED 2-1/2" PRESSURE GAUGE |
| **CROSSLAY #2** | | |
| PO00007712 | 1 | CROSSLAY #2 - 1-1/2" |
| PO00000024 | 1 | CROSSLAY #2 CAPACITY - 200 FEET OF 1-3/4" HOSE |
| PO00000032 | 1 | CROSSLAY #2 - DOUBLE STACK HOSE DESIGN |
| PO00024219 | 1 | 1-1/2" NST CHICKSAN SWIVEL |
| PO00006661 | 1 | CROSSLAY #2 PLUMBING - 2" STAINLESS STEEL PIPING |
| PO00006667 | 1 | 2" AKRON #8800 STAINLESS STEEL BALL VALVE |
| PO00006681 | 1 | PUSH/PULL CONTROL |
| PO00006712 | 1 | INNOVATIVE CONTROLS LIQUID FILLED 2-1/2" PRESSURE GAUGE |
| **CROSSLAY #3** | | |
| PO00007716 | 1 | CROSSLAY #3 - 2-1/2" |
| PO00000038 | 1 | CROSSLAY #3 CAPACITY - 200 FEET OF 2-1/2" HOSE |
| PO00000042 | 1 | CROSSLAY #3 - DOUBLE STACK HOSE DESIGN |
| PO00006743 | 1 | 2-1/2" NST CHICKSAN SWIVEL |
| PO00006746 | 1 | CROSSLAY #3 PLUMBING - 2-1/2" STAINLESS STEEL PIPING |
| PO00006750 | 1 | PUSH/PULL CONTROL |
| PO00006783 | 1 | INNOVATIVE CONTROLS LIQUID FILLED 2-1/2" PRESSURE GAUGE |
| PO00009198 | 1 | 2-1/2" AKRON #8800 STAINLESS STEEL BALL VALVE |
| **CROSSLAY/SPEEDLAY OPTIONS** | | |
| PO00011374 | 1 | VINYL CROSSLAY COVER |
| PO00011376 | 1 | CROSSLAY COVER RED IN COLOR |
| **AERIAL WATERWAY DISCHARGE** | | |
| PO00012681 | 1 | AERIAL WATERWAY DISCHARGE |
| PO00012685 | 1 | WATERWAY DISCHARGE PLUMBING - 4" STAINLESS STEEL |
| PO00012690 | 1 | 4" AKRON #8940 STAINLESS STEEL BALL VALVE |
| PO00012722 | 1 | AKRON HANDWHEEL GEAR VALVE CONTROL |
| PO00024059 | 1 | INNOVATIVE CONTROLS NITE-GLO WHITE/BLUE 2-1/2" PRESSURE GAUGE - WATERWAY |
| **PUMP MODULE AND OPTIONS** | | |
| PO00010791 | 1 | PUMP INSTALLATION - |
| PO00016063 | 1 | SIDE MOUNT PUMP MODULE |
| PO00000007 | 1 | PUMP MODULE - ALUMINUM CONSTRUCTION |
| **RUNNINGBOARD STEPS AND WALKWAY** | | |
| PO00012589 | 1 | SLIDE-OUT STEP - DRIVER PUMP OPERATOR'S PANEL |
| PO00015375 | 1 | RUNNING BOARD STEPS |
| **PUMP PANEL AND OPTIONS** | | |
| PO00016114 | 1 | SIDE MOUNT PUMP PANEL |
| PO00000095 | 1 | SIDE MOUNT PANELS - BLACK LINE-X COATED |
| PO00000128 | 1 | VERTICALLY HINGED GAUGE PANEL |
| PO00000132 | 1 | OFFICER SIDE VERTICALLY HINGED PUMP ACCESS DOOR |
| PO00010829 | 1 | PANEL FASTENERS |
| PO00010831 | 1 | CAPS AND ADAPTERS SAFETY TETHER - CABLES |
| PO00010832 | 1 | PUMP PANEL DISCHARGE / SUCTION TRIM PLATES - HIGH POLISHED |
| PO00010833 | 1 | DISCHARGE GAUGE TRIM BEZELS |
| PO00010834 | 1 | IDENTIFICATION PLATES |
| PO00012156 | 1 | PUMP OPERATOR'S PANEL LIGHT SHIELD |
| PO00012163 | 1 | TECNIQ E18 LED LIGHTS |
| PO00012176 | 1 | OFFICER SIDE PUMP PANEL LIGHT SHIELD |
| PO00012183 | 1 | TECNIQ E18 LED LIGHTS |
| PO00012573 | 1 | AIR HORN CONTROL BUTTON ON PUMP PANEL |
| PO00012576 | 1 | 3/8" PUMP BY-PASS COOLER ON PUMP PANEL |
| PO00011409 | 1 | PUMP PRESSURE & VACUUM TEST PORTS |
| PO00011423 | 1 | 4" INNOVATIVE CONTROLS MASTER PRESSURE AND COMPOUND GAUGES |
| PO00011442 | 1 | PRESSURE & COMPOUND GAUGE RANGES - SINGLE STAGE |
| **PUMP CERTIFICATION** | | |
| PO00025813 | 1 | PUMP THIRD PARTY CERTIFICATION |
| **PUMPER WATER TANK AND OPTIONS** | | |
| PO00023886 | 1 | TANK DESCRIPTION AND MOUNT |
| **AERIAL WATER TANK & OPTIONS** | | |
| \*\*\*SPECIAL: SP00000422 | 1 | WATER TANK CAPACITY - 650 GALLONS |
| **WATER TANK CONSTRUCTION** | | |
| PO00027025 | 1 | WATER TANK CONSTRUCTION - POLY |
| **WATER TANK LEVEL GAUGE/S** | | |
| PO00007590 | 1 | FIRE RESEARCH TANK VISION #WLA300-A00 LED WATER TANK GAUGE - PRIMARY |
| PO00007597 | 1 | FIRE RESEARCH WATER LEVEL GAUGE - 1/4" NPT PRESSURE TRANSDUCER |
| PO00007599 | 1 | FIRE RESEARCH WATER LEVEL GAUGE - WLA290 RELAY DRIVER FOR MONSTER LIGHT |
| PO00007605 | 1 | WHELEN PSTANK2 MONSTER WATER LEVEL GAUGES - EACH SIDE OF CAB |
| **BODY MODEL AND DESIGN** | | |
| PO00023833 | 1 | GENERAL COMPARTMENT |
| **BODY FENDER AND OPTIONS** | | |
| PO00009648 | 1 | FENDER WITH STORAGE OPTIONS |
| PO00026253 | 1 | DRIVER FORWARD FENDER - TRIPLE STORAGE SLOT |
| PO00026257 | 1 | DRIVER REARWARD FENDER - DOUBLE STORAGE SLOT |
| PO00026259 | 1 | OFFICER FORWARD FENDER - TRIPLE STORAGE SLOT |
| PO00026262 | 1 | OFFICER REARWARD FENDER - TRIPLE STORAGE SLOT |
| **AERIAL 103' "TUFF TRUCK" COMPARTMENTATION** | | |
| \*\*\*SPECIAL: SP00038009 | 1 | OFFICER SIDE COMPARTMENTATION |
| \*\*\*SPECIAL: SP00038010 | 1 | DRIVER SIDE COMPARTMENTATION |

|  |  |  |
| --- | --- | --- |
| **DRIVER SIDE AND OFFICER SIDE COMPARTMENT DOORS** | | |
| PO00000283 | 1 | AMDOR ROLL-UP DOORS - PAINTED FINISH |
| PO00009734 | 12 | PAINTED ROLL-UP DOORS - PAINTED CURTAIN & TOP GUTTER |
| PO00009727 | 12 | PROTECTION PANELS FOR ROLL-UP DOORS |
| PO00015348 | 1 | COMPARTMENT FLOORS |
| **BODY EXTERIOR** | | |
| PO00012483 | 1 | TREAD PLATE OVERLAY - FRONT OF BODY |
| PO00015351 | 1 | PAINTED REAR BODY PANEL |
| \*\*\*SPECIAL: SP00010600 | 1 | MITERED REAR BODY CORNERS |
| PO00027030 | 1 | BODY RUB RAILS - C-CHANNEL |
| PO00009797 | 1 | ALUMINUM WHEEL WELL LINERS |
| PO00009705 | 1 | POLISHED ALUMINUM FENDERETTES |
| PO00010934 | 1 | REAR MUD FLAPS |
| **BODY HANDRAILS AND STEPS** | | |
| PO00015394 | 1 | "STRAIGHT SHOT" EXTRUDED ALUMINUM BODY HANDRAILS |
| PO00011511 | 1 | INNOVATIVE CONTROLS LIGHTED STEPS – DRIVER SIDE FRONT BODY |
| PO00011517 | 1 | INNOVATIVE CONTROLS LIGHTED STEPS – OFFICER SIDE FRONT BODY |
| **REAR TOW EYES AND HITCH OPTIONS** | | |
| PO00015454 | 1 | PAINTED REAR TOW EYES BELOW BODY |
| **HOSEBED AND OPTIONS** | | |
| PO00015458 | 1 | "STRAIGHT SHOT" HOSE BED |
| PO00015470 | 1 | ALUMINUM HOSE BED FLOORING |
| PO00023838 | 1 | HOSE BED COVER - VINYL WITH VELCRO |
| PO00023841 | 1 | HOSE BED COVER – RED IN COLOR |
| **GROUND LADDER AND STORAGE** | | |
| PO00014876 | 1 | CENTER LADDER STORAGE TUNNEL |
| PO00014898 | 1 | LADDER STORAGE COMPARTMENT DOOR – PAINTED ROLL-UP DOOR |
| PO00014903 | 1 | STAINLESS STEEL LADDER LOCK SYSTEM |
| **GROUND LADDERS** | | |
| PO00021883 | 1 | ALCO-LITE PRL-14 14' ROOF LADDER WITH FOLDING HOOKS |
| PO00021928 | 1 | ALCO-LITE AEL-10 10' ATTIC EXTENSION LADDER |
| PO00021981 | 1 | DUO-SAFETY 1200-A 35' 2-SECTION EXTENSION LADDER |
| PO00021984 | 1 | DUO-SAFETY 900-A 24' 2-SECTION EXTENSION LADDER |
| PO00021994 | 2 | DUO-SAFETY 875-A 16' ROOF LADDER WITH FOLDING HOOKS |
| **PIKE POLES AND PIKE POLE STORAGE** | | |
| PO00023728 | 6 | PIKE POLE TUBES |
| PO00012525 | 1 | FIRE HOOKS UNLIMITED PIKE POLES 2-6', 2-8', 2-10' WITH FIBERGLASS HANDLE |
| **ADJUSTABLE SHELVES** | | |
| PO00020736 | 1 | ALUMINUM STRUT CHANNEL FOR FUTURE SHELVING |
| PO00020764 | 1 | ALUMINUM STRUT, LOCATED L-1 |
| PO00020765 | 1 | ALUMINUM STRUT, LOCATED L-2 |
| PO00020766 | 1 | ALUMINUM STRUT, LOCATED L-3 |
| PO00020767 | 1 | ALUMINUM STRUT, LOCATED L-4 |
| PO00020768 | 1 | ALUMINUM STRUT, LOCATED L-5 |
| PO00020771 | 1 | ALUMINUM STRUT, LOCATED R-1 |
| PO00020772 | 1 | ALUMINUM STRUT, LOCATED R-2 |
| PO00020773 | 1 | ALUMINUM STRUT, LOCATED R-3 |
| PO00020774 | 1 | ALUMINUM STRUT, LOCATED R-4 |
| PO00020775 | 1 | ALUMINUM STRUT, LOCATED R-5 |
| **AERIAL DEVICE MODEL** | | |
| PO00023695 | 1 | 140" TRAVEL HEIGHT |
| PO00012872 | 1 | 103' "TUFF TRUCK" AERIAL LADDER |
| **AERIAL LADDER - DESIGN AND FEATURES** | | |
| PO00012907 | 1 | 103' AERIAL LADDER GENERAL INTENT & DESIGN STANDARDS |
| PO00012928 | 1 | MOUNTING OF AERIAL |
| PO00012936 | 1 | HEIGHT AND REACH - 103' 4-SECTION HD AERIAL LADDER |
| PO00012952 | 1 | MATERIAL STANDARDS |
| **AERIAL HYDRAULIC SYSTEM** | | |
| PO00012962 | 1 | 103' HD "TUFF TRUCK" AERIAL LADDER HYDRAULIC SYSTEM |
| PO00012980 | 1 | PARKER HOSE KIT - 4 JACK UNIT |
| PO00012985 | 1 | HYDRAULIC PUMP - PRESSURE COMPENSATED |
| PO00012988 | 1 | HYDRAULIC RESERVOIR - 40 GALLON |
| PO00012996 | 1 | HYDRAULIC OIL - REGULAR A/W 46 |
| PO00013004 | 1 | DIVERTER VALVE |
| PO00013012 | 1 | OUTRIGGER HYDRAULIC CONTROL VALVE |
| PO00013019 | 1 | ELECTRIC TURNTABLE HYDRAULIC CONTROL VALVE |
| PO00013031 | 1 | HYDRAULIC SYSTEM FILTRATION |
| PO00013068 | 1 | 103' H.D. AERIAL LADDER EMERGENCY HYDRAULIC PUMP (EPU) |
| PO00013087 | 1 | HOT SHIFT PTO WITH CONTROLS IN CAB |
| PO00013091 | 1 | FAST IDLE CONTROL FOR ALL AERIAL DEVICES |
| **AERIAL MOTION CONTROL SYSTEM** | | |
| PO00013040 | 1 | 4-OUTRIGGER REAR MOUNT LADDER - "IQAN" MOTION CONTROL SYSTEM - ELECTRIC CONTROLS AT TURNTABLE |
| PO00013051 | 1 | HYDRAULIC PUMP PRESSURE - DISPLAY |
| PO00013052 | 1 | ELEVATION ANGLE OF LADDER - DISPLAY |
| PO00013053 | 1 | VERTICAL HEIGHT OF LADDER - DISPLAY |
| PO00013054 | 1 | DEGREE OF ROTATION FROM VEHICLE CENTERLINE - DISPLAY |
| PO00013055 | 1 | E-ZONE CAB & BODY AVOIDANCE WARNING - DISPLAY |
| PO00013056 | 1 | E-ZONE SHORT JACK WARNING - DISPLAY |
| PO00013057 | 1 | CRADLE ALIGNMENT MESSAGE - DISPLAY |
| PO00013060 | 1 | E-SPEED LADDER TIP SPEED CONTROL - DISPLAY |
| PO00013061 | 1 | E-CUSH RAMP CONTROL FOR ELEVATION - DISPLAY |
| PO00013062 | 1 | E-CUSH RAMP CONTROL FOR EXTENSION & RETRACTION - DISPLAY |
| PO00013063 | 1 | WARNING MESSAGES - TURNTABLE ONLY |
| PO00013283 | 1 | OUTRIGGER CONTROLS |
| PO00013584 | 1 | IQAN INCLINOMETER |
| PO00013585 | 1 | IQAN MOMENT LOAD INDICATOR |
| PO00013586 | 1 | IQAN E-CUSH CONTROL ELEVATION SYSTEM |
| PO00013640 | 1 | IQAN "E-SPEED" SAFETY SYSTEM |
| PO00013645 | 1 | IQAN “E-ZONE" ROTATION SAFETY SYSTEM |
| PO00013646 | 1 | IQAN "E-ZONE" CAB & BODY PROXIMITY SYSTEM |
| PO00013674 | 1 | IQAN EXTENSION SYSTEM STRING POTENTIOMETER |
| PO00013675 | 1 | IQAN "E-CUSH" EXTENSION/RETRACTION SYSTEM |
| PO00014229 | 1 | IQAN "CREEPER CONTROLS" AT LADDER TIP |
| **AERIAL TORQUEBOX** | | |
| PO00013100 | 1 | 103' HD "TUFF TRUCK" AERIAL LADDER TORQUE BOX |
| PO00013193 | 1 | IQAN OUTRIGGER STRING POTENTIOMETER |
| PO00013554 | 1 | AERIAL TRAVEL SUPPORT |
| **AERIAL OUTRIGGERS** | | |
| PO00024052 | 1 | OUTRIGGERS NOT STOWED INDICATOR ON DASH |
| PO00015370 | 1 | 1/2 WIDTH STAINLESS STEEL OUTRIGGER COVER PANEL |
| PO00013125 | 1 | 103 HD "TUFF TRUCK" AERIAL OUTRIGGERS – 12’ JACKSPREAD |
| PO00013149 | 1 | 103' HD "TUFF TRUCK" LADDER OUTRIGGERS - HORIZONTAL CYLINDERS |
| PO00013176 | 1 | HD LADDER OUTRIGGERS - VERTICAL CYLINDERS & EXTENDED STROKE |
| PO00013199 | 1 | OVERSIZED OUTRIGGER/JACK FOOT PADS |
| PO00013207 | 1 | OUTRIGGER INTERLOCK SYSTEM & ALARM |
| PO00013276 | 1 | OUTRIGGER SCOTCHLITE - RED/YELLOW CHEVRON |
| PO00013305 | 1 | OUTRIGGER LEVEL SIDE TO SIDE |
| PO00013306 | 1 | OUTRIGGER LEVEL FORE & AFT |
| **AERIAL OUTRIGGER WARNING LIGHTS** | | |
| PO00013223 | 1 | AKRON LED OUTRIGGER LAMPS |
| PO00013230 | 1 | LED OUTRIGGER GROUND LIGHTS - FIRETECH P500 |
| **AERIAL TURNTABLE** | | |
| PO00013315 | 1 | 103' H.D. AERIAL LADDER TURNTABLE |
| PO00013335 | 1 | TURNTABLE DECK - SMOOTH ALUMINUM WITH BLACK LINE-X COATING |
| PO00013342 | 1 | HEEL PIN STEP ON TURNTABLE |
| PO00026389 | 1 | TURNTABLE HANDRAILS |
| PO00013353 | 1 | HEEL PINS |
| PO00013363 | 1 | STAINLESS STEEL CRADLE ALIGNMENT ARROWS ON TURNTABLE |
| PO00013367 | 1 | SAFETY CHAINS BETWEEN TURNTABLE HANDRAIL |
| PO00013378 | 1 | 103' H.D. AERIAL LADDER TURNTABLE SWIVEL |
| PO00013403 | 1 | IQAN SWIVEL ROTATION ENCODER |
| **AERIAL LADDER CONSTRUCTION** | | |
| PO00013408 | 1 | 103' H.D. LADDER CONSTRUCTION |
| PO00013433 | 1 | 103' H.D. 4-SECTION LADDER DIMENSIONS |
| PO00013468 | 1 | PHOTOLUMINESCENT RUNG COVERS |
| PO00013691 | 1 | LADDER CABLE/HOSE/WIRE ROUTING |
| **AERIAL DEVICE OPTIONS** | | |
| PO00013429 | 1 | STAINLESS STEEL EGRESS With TIP SKID GUARDS |
| PO00013470 | 1 | SINGLE PAIR FOLDING STEPS at LADDER TIP |
| PO00013477 | 1 | EGRESS PAINTING TO MATCH LADDER COLOR |
| PO00013480 | 1 | 8' FIRE HOOKS UNLIMITED PIKE POLE MOUNTED IN FLY SECTION |
| PO00013484 | 1 | PIKE POLE MOUNTED ON LEFT SIDE OF FLY SECTION |
| PO00013523 | 1 | ROOF LADDER MOUNT ON BASE SECTION |
| PO00013541 | 1 | 14' DUO-SAFETY 775A-14 ROOF LADDER PROVIDED – BASE section |
| PO00013545 | 1 | SPECIFIED ROOF LADDER MOUNTED ON RIGHT SIDE OF BASE section |
| PO00013546 | 1 | RESCUE EYELET ON LAST RUNG OF LADDER TIP |
| PO00013688 | 1 | backlit LADDER LEVEL INDICATOR at BASE SECTION |
| **AERIAL ELEVATION SYSTEM** | | |
| PO00013565 | 1 | 103' H.D. AERIAL LADDER ELEVATION SYSTEM |
| **AERIAL ROTATION SYSTEM** | | |
| PO00013612 | 1 | 103' H.D. AERIAL LADDER ROTATION SYSTEM |
| PO00013632 | 1 | ROTATION MOTOR AND BRAKE - 41" EXTERNAL BEARINGS |
| PO00013638 | 1 | SWING DRIVE ADJUSTMENT |
| **AERIAL EXTENSION SYSTEM** | | |
| PO00013652 | 1 | 103' H.D. AERIAL LADDER EXTENSION / RETRACTION SYSTEM |
| PO00013669 | 1 | EXTENSION CYLINDERS PAINTED LADDER PAINT COLOR |
| PO00013682 | 1 | LADDER SLIDE PADS |
| \*\*\*SPECIAL: SP00025290 | 1 | LADDER EXTENSION NUMBERS |
| **AERIAL LADDER 120-VOLT LIGHTING** | | |
| PO00013736 | 1 | 120-VOLT ELECTRICAL SYSTEM |
| PO00013738 | 1 | 120-VOLT NEMA 20 AMP RECEPTACLE at LADDER TIP |
| **AERIAL LADDER 12-VOLT LIGHTING** | | |
| PO00013560 | 1 | CRADLE ILLUMINATION LIGHTS - FIRETECH P500 LED |
| PO00013783 | 1 | HEEL PIN STEP LIGHTS - TECNIQ EON 3 LED LIGHTS |
| PO00013789 | 1 | TURNTABLE CONTROL CONSOLE LeD lighting |
| PO00013816 | 1 | TWO (2) FRC SOBRITE LED FLOOD LIGHTS at LADDER TIP |
| PO00013921 | 1 | LADDER WALKWAY ILLUMINATION LIGHTs |
| PO00013925 | 1 | CLEAR LADDER ILLUMINATION LIGHTS |
| PO00026135 | 1 | TURNTABLE CONSOLE STEP LIGHT |
| PO00025801 | 1 | TWO (2) FRC SOBRITE LED FLOOD LIGHTS ON LADDER BASE SECTION |
| **AERIAL LADDER TURNTABLE CONTROL CONSOLE** | | |
| PO00014152 | 1 | ladder CONTROL STATION |
| PO00014153 | 1 | CONSOLE LOCATion - left SIDE OF TURNTABLE |
| PO00014159 | 1 | PAINTED ALUMINUM TURNTABLE CONSOLE - MATCH LADDER |
| PO00025856 | 1 | IQAN MD4-10 DISPLAY TURNTABLE CONSOLE |
| \*\*\*SPECIAL: SP00027771 | 1 | AERIAL LADDER TURNTABLE CONTROL STATION - ADVANCED CONTROLS |
| \*\*\*SPECIAL: SP00027275 | 1 | LADDER SPEED CONTROL KNOB - TURNTABLE CONTROL CONSOLE |
| PO00014191 | 1 | "WATERWAY CHARGED" INDICATOR LIGHT - TURNTABLE CONSOLE |
| PO00014192 | 1 | AIRHORN CONTROL BUTTON - TURNTABLE CONTROL CONSOLE |
| PO00014193 | 1 | AERIAL HOURMETER - TURNTABLE CONTROL CONSOLE |
| PO00026156 | 1 | AERIAL FLOWMETER - TURNTABLE CONSOLE |
| PO00014218 | 1 | painted TURNTABLE CONSOLE COVER |
| **AERIAL COMMUNICATIONS** | | |
| PO00014268 | 1 | LADDER, FRC ACT 2-WAY COMMUNICATION SYSTEM - LOWER CONTROL |
| PO00014269 | 1 | LADDER, FRC ACT 2-WAY COMMUNICATION SYSTEM - UPPER SPEAKER/MIC |
| **AERIAL LADDER WATERWAY AND OPTIONS** | | |
| PO00014347 | 1 | 103' H.D. AERIAL LADDER WATERWAY SYSTEM |
| PO00027031 | 1 | WATERWAY INLET LOCATED AT OFFICER PUMP PANEL |
| PO00014372 | 1 | 103' H.D. AERIAL LADDER WATERWAY |
| PO00014395 | 1 | 4" HEEL PIN SWIVEL |
| PO00014404 | 1 | AUTOMATIC WATER DRAIN / VENT |
| PO00014405 | 1 | WATERWAY RELIEF VALVE |
| PO00014406 | 1 | REAR MOUNT AERIAL WATERWAY DRAIN - 1-1/2" VALVE |
| PO00014411 | 1 | AERIAL WATERWAY DRAIN CONTROL |
| PO00014412 | 1 | 4" NST REAR AERIAL WATERWAY INLET ADAPTER |
| PO00014447 | 1 | INNOVATIVE CONTROLS 2-1/2" GAUGE FOR AERIAL INLET |
| **AERIAL LADDER MONITOR AND OPTIONS** | | |
| PO00014502 | 1 | ELKHART #7250 SD EXM2 COBRA "RF" MONITOR |
| PO00014519 | 1 | ELKHART MONITOR CONTROLS With AUTO STOW |
| \*\*\*SPECIAL: SP00037091 | 1 | SELECTABLE WATERWAY TROLLEY |
| PO00014540 | 1 | ELKHART ST-194 QUAD STACKED TIPS (ELK-O-LITE) |
| \*\*\*SPECIAL: SP00021604 | 1 | LADDER ELECTRIC TFT VALVE UNDER MONITOR |
| PO00014546 | 1 | 2-1/2” NH GATED ELBOW LEFT HAND VALVE UNDER MONITOR |
| PO00014552 | 1 | "STORE FRONT BLITZ" DESCRIPTION |
| **AERIAL CAPACITIES** | | |
| PO00014775 | 1 | 103' H.D. AERIAL LADDER CAPACITIES |
| **AERIAL SPECIAL EQUIPMENT** | | |
| PO00014821 | 1 | AERIAL LADDER, MANUALS – two-(2) sets |
| **AERIAL TESTING - FINAL** | | |
| PO00014804 | 1 | FIRE DEPartment AERIAL FAMILIARIZATION PROVIDED BY FACTORY |
| PO00014805 | 1 | one-(1) day FACTORY FAMILIARIZATION |
| PO00014819 | 1 | AERIAL SERVICE |
| PO00014820 | 1 | WARNING DECALS |
| PO00014853 | 1 | 103' H.D. AERIAL LADDER CERTification & TESTING |
| **PAINT PROCESS** | | |
| PO00010847 | 1 | GENERAL PAINT DESCRIPTION |
| PO00014914 | 1 | GENERAL PRIMER & PREP DESCRIPTION |
| PO00014917 | 1 | GENERAL FINISH PAINT DESCRIPTION |
| PO00010852 | 1 | CUSTOM FINISH PAINT & PREP |
| **CAB PAINT** | | |
| PO00010851 | 1 | CUSTOM CAB PRIMER & PREP |
| PO00011729 | 1 | CUSTOM CAB UNDERSIDE PAINT - BLACK |
| PO00010853 | 1 | CUSTOM CAB BUFFING & FINISH |
| PO00004569 | 1 | CUSTOM CAB INTERIOR PAINT - TEXTURED GRAY |
| **BODY PAINT** | | |
| PO00014920 | 1 | BODY BUFFING & FINISH |
| PO00022128 | 1 | INSIDE / UNDERSIDE BODY PAINTED BLACK |
| PO00026354 | 1 | COMPARTMENT INTerior - MULTISPEC GRAY STONE |
| PO00004566 | 1 | SINGLE COLOR CUSTOM CAB PAINT SCHEME |
| **PUMP MODULE AND PLUMBING PAINT** | | |
| PO00022250 | 1 | PUMP PAINTED / UNPAINTED PLUMBING |
| **PAINT CODES AND COLORS** | | |
| PO00014945 | 1 | SINGLE COLOR BODY PAINT SCHEMe |
| **FINALIZATION** | | |
| PO00023890 | 1 | LADDER RUST INHIBITOR |
| PO00010855 | 1 | PINT OF TOUCH-UP PAINT |
| PO00014988 | 1 | FINALIZATION & DETAILING |
| **CHASSIS PAINT** | | |
| PO00004576 | 1 | CUSTOM CHASSIS GLOSS BLACK COLOR FRAME RAILS |
| **AERIAL DEVICE PAINT** | | |
| PO00024542 | 1 | aerial device paint - SILVER #FLNA95963 |
| PO00014958 | 1 | EXTENSION CYLINDERS PAINTED TO MATCH LADDER COLOR |
| PO00014964 | 1 | TORQUEBOX PAINT - BLACK |
| PO00014966 | 1 | OUTRIGGER PAINT - SILVER URETHABOND 104 |
| PO00014968 | 1 | TURNTABLE PAINT - LADDER COLOR |
| PO00014970 | 1 | TURNTABLE CONSOLE PAINT - LADDER COLOR |
| PO00014972 | 1 | LIFT CYLINDERS PAINT - LADDER COLOR |
| **CHEVRON STRIPING** | | |
| PO00009536 | 1 | REAR CHEVRON STRIPING |
| PO00012448 | 1 | ENTIRE REAR |
| PO00009540 | 1 | 6" FULL REAR ORALITE CHEVRON STRIPING |
| PO00024628 | 1 | RED & YELLOW ORALITE V98 |
| **MISCELANEOUS EQUIPMENT** | | |
| PO00026066 | 1 | MISCELLANEOUS EQUIPMENT |
| PO00011822 | 1 | ROAD SAFETY KITS |
| PO00000521 | 1 | TWO (2) ZICO #SAC-44 FOLDING WHEEL CHOCKS |
| **WARRANTY** | | |
| PO00023664 | 1 | KME WARRANTY STARTING ON IN-SERVICE DATE |
| **WARRANTY - STANDARD AND EXTENDED** | | |
| PO00026895 | 1 | GENERAL ONE (1) YEAR OR 24,000 MILES LIMITED WARRANTY |
| PO00026922 | 1 | REGULATED EMISSIONS SYSTEMS FIVE (5) YEARS OR CARB MILEAGE LIMITED WARRANTY |
| PO00026923 | 1 | ELECTRICAL ONE (1) YEAR OR 18,000 MILES LIMITED WARRANTY |
| PO00026939 | 1 | FRAME ASSEMBLY STRUCTURAL TEN(10) YEARS OR 100,000 MILES LIMITED WARRANTY |
| PO00026948 | 1 | FRAME RAIL CORROSION (ZINC PLATE AND POWDER COAT) TWENTY FIVE (25) YEARS OR 150,000 MILES LIMITED WARRANTY |
| PO00026951 | 1 | AERIAL LADDER STRUCTURE TWENTY (20) YEARS OR 100,000 MILES LIMITED WARRANTY |
| PO00026953 | 1 | AERIAL TORQUE BOX STRUCTURE FIFTEEN (15) YEARS OR 100,000 MILES LIMITED WARRANTY |
| PO00026954 | 1 | AERIAL LEAK-FREE HYDRAULICS THREE (3) YEARS OR 48,000 MILES LIMITED WARRANTY |
| PO00026956 | 1 | BODY STRUCTURal (ALUMINUM) TEN (10) YEARS OR 100,000 MILES LIMITED WARRANTY |
| PO00026977 | 1 | PAINT AND FINISH (EXTERIOR CLEAR COATED) TEN (10) YEARS LIMITED WARRANTY |
| PO00026981 | 1 | PLUMBING AND PIPING (STAINLESS STEEL) TEN (10) YEARS OR 100,000 MILES LIMITED WARRANTY |
| PO00026983 | 1 | AERIAL WATERWAY TEN (10) YEARS OR 100,000 MILES LIMITED WARRANTY |
| PO00022661 | 1 | five (5) YEAR CUMMINS BASE WARRANTY |
| PO00022665 | 1 | five (5) YEAR ALLISON EVS TRANSMISSION WARRANTY |
| PO00022980 | 1 | three (3) YEAR COOLING SYSTEM WARRANTY - CUSTOM |
| PO00022978 | 1 | three (3) year SHEPPARD STEERING GEAR STANDARD WARRANTY |
| PO00022678 | 1 | five (5) YEAR MERITOR SINGLE AXLE REAR WARRANTY |
| PO00022681 | 1 | three (3) YEAR MERITOR ABS WARRANTY |
| PO00022701 | 1 | ten (10) year PAINT FINISH WARRANTY |
| PO00022702 | 1 | five (5) YEAR LETTERING WARRANTY |
| PO00022703 | 1 | one (1) YEAR BRIGHTWORK WARRANTY |
| PO00022981 | 1 | ten (10) YEAR STAINLESS STEEL PIPING WARRANTY |
| PO00024719 | 1 | five (5) year FRONT SUSPENSION HENDRICKSON STEERTEK warranty |
| PO00022711 | 1 | One (1) year hendrickson REAR SUSPENSION warranty |
| PO00022973 | 1 | LIFETIME POLY TANK WARRANTY |
| PO00022735 | 1 | five (5) year HALE FIRE PUMP WARRANTY FULL LABOR |
| PO00022989 | 1 | CLASS 1 PRODUCT WARRANTY |
| PO00022764 | 1 | ten (10) year ELKHART HEAVY DUTY VALVE warranty |
| PO00022983 | 1 | two (2) year CLASS 1 ELECTRICAL PRODUCT WARRANTy |
| PO00022987 | 1 | six (6) year VALOR SEATING wARRANTY |
| PO00010937 | 1 | CORROSION TREATMENT |
| PO00022954 | 1 | three (3) year HARRISON 6-8-10 MSV-MAS-MCR-MDS EXTENDED WARRANTY |
| **SUPPORT, DELIVERY, INSPECTIONS, MANUALS** | | |
| PO00024053 | 1 | ADDITIONAL ITEMS SHIPPED WITH VEHICLE |